# Grove_Sunlight_Sensor

<img src=https://statics3.seeedstudio.com/images/product/101020089%201.jpg width=300><img src=https://statics3.seeedstudio.com/product/101020089%201_01.jpg width=300>

[Grove - Sunlight Sensor](https://www.seeedstudio.com/Grove-Sunlight-Sensor-p-2530.html)

Grove - Sunlight Sensor is a multi-channel digital light sensor, which has the ability to detect UV-light, visible light and infrared light.

This device is based on SI1145, a new sensor from SiLabs. The Si1145 is a low-power, reflectance-based, infrared proximity, UV index and ambient light sensor with I2C digital interface and programmable-event interrupt output. This device offers excellent performance under a wide dynamic range and a variety of light sources including direct sunlight.

For more information please visit [wiki](http://wiki.seeedstudio.com/Grove-Sunlight_Sensor/).

----

This demo is licensed under [The MIT License](http://opensource.org/licenses/mit-license.php). Check LINCESE for more information.<br>

Contributing to this software is warmly welcomed. You can do this basically by<br>
[forking](https://help.github.com/articles/fork-a-repo), committing modifications and then [pulling requests](https://help.github.com/articles/using-pull-requests) (follow the links above<br>
for operating guide). Adding change log and your contact into file header is encouraged.<br>
Thanks for your contribution.

Seeed Studio is an open hardware facilitation company based in Shenzhen, China. <br>
Benefiting from local manufacture power and convenient global logistic system, <br>
we integrate resources to serve new era of innovation. Seeed also works with <br>
global distributors and partners to push open hardware movement.<br>



[![Analytics](https://ga-beacon.appspot.com/UA-46589105-3/Grove_Sunlight_Sensor)](https://github.com/igrigorik/ga-beacon)
