## OLED_Display_128X64
![image](https://raw.githubusercontent.com/SeeedDocument/Grove_OLED_Display_0.96/master/images/Grove-OLED-0.96.png)

LED 128×64 Display module is an OLED monochrome 128×64dot matrix display module with Grove 4pin I2C Interface.Comparing to LCD, OLED screens are way more competitive, which has a number of advantages such as high brightness, self-emission, high contrast ratio, slim / thin outline, wide viewing angle, wide temperature range, and low power consumption. It has bigger screen so that it can display more contents than the OLED 96×96. 

For more information, please refer to [Grove_OLED_Display_128X64][1]

----
This software is written by Frankie Chu for seeed studio and is licensed under The GPL v2 License.<br>

Contributing to this software is warmly welcomed. You can do this basically by<br>
[forking](https://help.github.com/articles/fork-a-repo), committing modifications and then [pulling requests](https://help.github.com/articles/using-pull-requests) (follow the links above<br>
for operating guide). Adding change log and your contact into file header is encouraged.<br>
Thanks for your contribution.

Seeed is a hardware innovation platform for makers to grow inspirations into differentiating products. By working closely with technology providers of all scale, Seeed provides accessible technologies with quality, speed and supply chain knowledge. When prototypes are ready to iterate, Seeed helps productize 1 to 1,000 pcs using in-house engineering, supply chain management and agile manufacture forces. Seeed also team up with incubators, Chinese tech ecosystem, investors and distribution channels to portal Maker startups beyond.


[1]:http://wiki.seeed.cc/Grove-OLED_Display_0.96inch/


[![Analytics](https://ga-beacon.appspot.com/UA-46589105-3/OLED_Display_128X64)](https://github.com/igrigorik/ga-beacon)
