# Adafruit INA219 Library [![Build Status](https://github.com/adafruit/Adafruit_INA219/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit_INA219/actions)[![Documentation](https://github.com/adafruit/ci-arduino/blob/master/assets/doxygen_badge.svg)](http://adafruit.github.io/Adafruit_INA219/html/index.html)

<a href="https://www.adafruit.com/products/904"><img src="assets/board.jpg" width="500px" /></a>

This is a library for the Adafruit INA219 high side DC current sensor boards:
  * https://www.adafruit.com/products/904
  * https://www.adafruit.com/product/3650
 
Check out the links above for our tutorials and wiring diagrams. This chip uses I2C to communicate.

To install, use the Arduino Library Manager and search for 'Adafruit INA219' and install the library.

Adafruit invests time and resources providing this open source code, please support Adafruit and open-source hardware by purchasing products from Adafruit!

Written by Ktown for Adafruit Industries.
MIT license, all text above must be included in any redistribution
